

Question 14

Try Static NAT, Dynamic NAT and PAT to translate Ips


Make the below given network




Now configure swith and create vlan’s




Now configure the router to communicate between inter vlan




Now if you try to ping another network it works.



Now configure for Static NAT



The packet’s source IP after nat




Dynamic nat

Create a pool of public nat



Add source list and add nat to the network





Now you can check the arp packet has assigned public ip

